Room CO2  
Monitoring

Carbon Dioxide (CO2) Monitor

PART 1 – GENERAL

1. RELATED DOCUMENTS
   1. Drawings and general provisions of the Contract, including General and Supplementary General Conditions and other Division 01 Specification Sections, apply to this Section

PART 2 – PRODUCTS

* 1. Wall Mount CO2 Monitor (S&S Middle East RSCO2 Range)
     1. Product supplied shall be a wall mount carbon dioxide (CO2) monitor rated for indoor environments.
     2. CO2 monitor range shall be available with Bacnet MS/TP or Modbus RTU communication protocols options.
     3. System shall have internal volt free relays & 0-10V output to activate ventilation equipment and warning alarms upon reaching alarm thresholds.
     4. CO2 monitor range shall be available with blank, LED or display screen options.
     5. CO2 monitor range shall be available as 24VAC/DC or 230VAC powered.
     6. System shall have an operating temperature range: -10°C to 50°C.
     7. System shall be 5.95” x 4.37” x 1.87”
     8. Acceptable product range: S&S Middle East RSCO2

PART 3 – EXECUTION

* 1. INSTALLATION
     1. Sensors must be installed in compliance with the manufacturer's guidelines.
     2. Install wiring and conduit to prevent interference with other systems.
     3. Ensure accessibility for future sensor maintenance and calibration.